[DIAGNOSTICA]
CAPTION=DIAGNOSTIC
MAPPAERRORI.0=ERROR CODE
MAPPAERRORI.1=DIAGNOSTIC DEVICE
MAPPAERRORI.2=ERROR TYPE
MAPPAERRORI.3=STATE
BOXCAL.CAPTION=SETTING
BOXAGGIUNTIVI.CAPTION=OTHER PARAMETERS
CONTESTO.0=P1 Pressure =
CONTESTO.1=MAP Pressure =
CONTESTO.2=TPS =
CONTESTO.3=PRECAT1 =
CONTESTO.4=RPM =
CONTESTO.5=PETROL TON =
CONTESTO.6=GAS TON =
CONTESTO.7=GAS TEMPERATURE =
CONTESTO.8=SUPPLY STATE =
CONTESTO.9=EVENT COUNTER =
CONTESTO.10=H2O TEMPERATURE =
MISURA.0=mBar
MISURA.1=%
MISURA.2=mV
MISURA.3=°C
MISURA.4=ms
ALIMENTAZIONE.0=SWITCHED ON
ALIMENTAZIONE.1=GAS Mode
ALIMENTAZIONE.2=Changeover
ALIMENTAZIONE.3=Petrol Mode
LABDATI.0=N1
LABDATI.1=Q1
LABDATI.2=N2
LABDATI.3=Q2
LABDATI.4=MinConv
LABDATI.5=MaxConv
LABDATI.6=MinPhis
LABDATI.7=MaxPhis
LABDATI.8=Activate the buzzer while recognising the error
LABDATI.9=Activate the rechangeover while recognising the error
LABDATI.10=Max error detection Time
LABDATI.11=Light indicator check
LABDATI.12=T. detect. err. at 800 rpm
LABCAL.0=Diagnosticable devices enable:
LABDIA.0=Number of errors found
ABILITODISABILITO.0=ENABLE DEFAULT
ABILITODISABILITO.1=&DISABLE ALL
CONTESTOASSOCIATO.CAPTION=Associated context
INTERVENTO.CAPTION=Suggested operation
SEGNALAZIONE1.0=Not correct data!
SEGNALAZIONE1.1=TURN THE IGNITION KEY OFF AND THEN ON AGAIN TO RESTORE THE INITIAL CONDITIONS.
SEGNALAZIONE1.2=THIS OPTION NOT ENABLE LAMBDA OXIGEN SENSOR DIAGNOSTIC.
SEGNALAZIONE1.3=DIAGNOSTIC NOT CHANGEABLE : RELATED DATABASE DOES NOT EXIST
SEGNALAZIONE1.4=TO MAKE THE MODIFICATIONS EFFECTIVE YOU HAVE TO REPROGRAM THE ECU WHEN YOU EXIT FROM THIS SCREEN.
SEGNALAZIONE1.5=TO MANAGE THIS ERROR IS NECESSARY A SOFTWARE VERSION ON THE ECU >= xx
SEGNALAZIONE1.6=DIAGNOSTIC REPORT HAS BEEN SAVED IN "
SEGNALAZIONE1.7=DIAGNOSTIC NOT CHANGEABLE: SOFTWARE OR ECU NOT COMPATIBLE
[ERRORE_DISPOSITIVO]
ERRORE_0=Signal value out of the maximum range
ERRORE_1=Signal value out of the minimum range
ERRORE_2=No signal present
ERRORE_3=Not reasonable signal
STATO_0=Line test in progress
STATO_1=Error recorded
STATO_2=Filtered error
STATO_3=Wait for the first check of state error previously indicated as present
STATO_9=Present error
[P0190]
NOME=Petrol Pressure Sensor
U_MIS=mbar
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check the Sensor connector
DESCRIZIONE0_2=Check the absence of short-circuit between the Sensor wire and the positive supply
DESCRIZIONE0_3=Check Sensor setting
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE1_1=Check the Sensor connector
DESCRIZIONE1_2=Check the absence of short-circuit between the sensor wire and the negative supply
DESCRIZIONE1_3=Check Sensor setting
DESCRIZIONE1_4=Replace XXX ECU.
DESCRIZIONE2_1=Check the Sensor connector
DESCRIZIONE2_2=Check the Sensor wire continuity from the taking point to the XXX ECU.
DESCRIZIONE2_3=Check Sensor setting
DESCRIZIONE3_1=Check Sensor setting
DESCRIZIONE3_2=Replace XXX ECU.
[P1105]
NOME=MAP Sensor
U_MIS=mbar
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check the MAP sensor connector
DESCRIZIONE0_2=Check the absence of short-circuit between the MAP signal wire and the positive supply
DESCRIZIONE0_3=Replace the MAP sensor
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE1_1=Check the MAP sensor connector
DESCRIZIONE1_2=Check the absence of short-circuit between the MAP signal wire and the negative supply
DESCRIZIONE1_3=Check the MAP signal wire continuity from the sensor connector (or taking point) to XXX ECU connector.
DESCRIZIONE1_4=Replace the MAP sensor connector
DESCRIZIONE1_5=Replace XXX ECU.
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check the MAP sensor setting
DESCRIZIONE3_2=If you have a not-reasonable-error on P1 pressure sensor, follow the same indications suitable for the P1190 error
DESCRIZIONE3_3=If you have an error on TPS throttle potentiometer, follow the same indications suitable for the P1120 error
DESCRIZIONE3_4=If you have an error on sensors supply tension, follow the same indications suitable for the P1608 error
DESCRIZIONE3_5=Replace the MAP sensor
DESCRIZIONE3_6=Replace XXX ECU.
[P1115]
NOME=TH2O Sensor
U_MIS=°C
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check absence of short-circuit between the TH2O signal wire and the negative supply
DESCRIZIONE0_2=Replace XXX ECU.
DESCRIZIONE1_1=Check the welding in the taking point of the TH2O signal
DESCRIZIONE1_2=Check the absence of short-circuit between the TH2O signal wire and the positive supply
DESCRIZIONE1_3=Check the TH20 signal wire continuity from the sensor connector (or signal taking point) to XXX ECU connector.
DESCRIZIONE1_4=Replace XXX ECU.
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check the TH2O sensor setting
DESCRIZIONE3_2=If you have a not-reasonable-error on gas temperature sensor too, follow the same indications suitable for the P1180 error
DESCRIZIONE3_3=If you have an error on sensor supply tension too, follow the same indications wuitable for the P1608 error
DESCRIZIONE3_4=Replace XXX ECU.
[P1120]
NOME=TPS Sensor
U_MIS=%
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check the absence of short-circuit between the TPS signal wire and the positive supply
DESCRIZIONE0_2=Replace XXX ECU.
DESCRIZIONE1_1=Check the right connection of the TPS signal wire
DESCRIZIONE1_2=Check the absence of short-circuit between the TPS signal wire and the negative supply
DESCRIZIONE1_3=Check the TPS signal wire continuity from the sensor connector (or signal taking point) to XXX ECU connector.
DESCRIZIONE1_4=Replace XXX ECU.
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check the TPS sensor setting
DESCRIZIONE3_2=If you have an error on sensor supply tension, follow the same indications suitable for the P1608 error
DESCRIZIONE3_3=Replace XXX ECU.
[P1130]
NOME=PRECAT1 Signal
U_MIS=mV
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check that Lambda oxigen sensor signal had been correctly taken
DESCRIZIONE0_2=Check the absence of short-circuit between the PRECAT1 Lambda oxigen sensor signal wire and the positive supply
DESCRIZIONE0_3=Replace XXX ECU.
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check that Lambda oxigen sensor signal has been correctly taken
DESCRIZIONE3_2=Check the absence of short-circuit between the precat1 Lambda oxigen sensor signal wire and the negative supply.
DESCRIZIONE3_3=Check the sensor setting
DESCRIZIONE3_4=Replace XXX ECU.
[P1150]
NOME=PRECAT2 Signal
U_MIS=mV
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check that Lambda oxigen sensor signal had been correctly taken
DESCRIZIONE0_2=Check the absence of short-circuit between the PRECAT2 Lambda oxigen sensor signal wire and the positive supply
DESCRIZIONE0_3=Replace XXX ECU.
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check that Lambda oxigen sensor signal had been correctly taken
DESCRIZIONE3_2=Check the absence of short-circuit between the PRECAT2 Lambda oxigen sensor signal wire and the negative supply
DESCRIZIONE3_3=Check the sensor setting.
DESCRIZIONE3_4=Replace XXX ECU.
[P1131]
NOME=PRECAT1 ground
U_MIS=mV
U_MISC=mV
U_MIT=s
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check the absence of short-circuit between the PRECAT1L signal wire and the ground signal.
DESCRIZIONE3_2=Check the PRECAT1L signal wire continuity from the sensor to XXX ECU connector.
DESCRIZIONE3_3=Check that Lambda oxigen sensor ground had been correctly taken.
DESCRIZIONE3_4=Replace XXX ECU.
[P1151]
NOME=PRECAT2 ground
U_MIS=mV
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=NOT SUPPORTED
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=Check the absence of short-circuit between the PRECAT2L signal wire and the ground signal.
DESCRIZIONE3_1=Check that Lambda oxigen sensor PRECAT2 ground had been correctly taken.
DESCRIZIONE3_2=Check that Lambda oxigen sensor ground had been correctly taken.
DESCRIZIONE3_3=Replace XXX ECU.
[P1170]
NOME=Self-adapting maps threshold
U_MIS=
U_MISC=%
U_MIT=s
DESCRIZIONE0_1=NOT SUPPORTED
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check maps self-adapting parameters
DESCRIZIONE3_2=If you have an error on gas injectors control,  follow the same indications suitable for error P1201, P1202, P1203, P1204, P1205, P1206, P1207, P1208.
DESCRIZIONE3_3=If you have an error on petrol injectors inlet, follow the same indications suitable for error P1263, P1266, P1269, P1272, P1275, P1278, P1281, P1284.
DESCRIZIONE3_4=If you have an error on MAP pressure sensor, follow the same indications suitable for error P1105.
[P2531]
NOME=Key contact
U_MIS=%
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=NOT SUPPORTED
DESCRIZIONE1_1=Check correct connection of the VCH signal.
DESCRIZIONE1_2=Check VCH signal wire continuity from the sensor connector (or taking point signal) to XXX ECU connector.
DESCRIZIONE1_3=Replace XXX ECU.
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1173]
NOME=Actuators tension supply
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check wiring on Gas and Solenoid valves injectors supply.
DESCRIZIONE0_2=Check the absence of short-circuit between the actuators relay wiring and the positive supply.
DESCRIZIONE0_3=Replace XXX ECU.
DESCRIZIONE1_1=Check wiring on Gas and Solenoid valves injectors supply.
DESCRIZIONE1_2=Check the absence of short-circuit between the actuators relay wiring and the ground.
DESCRIZIONE1_3=Replace XXX ECU.
DESCRIZIONE2_1=Check wiring on Gas and Solenoid valves injectors supply.
DESCRIZIONE2_2=Check the absence of short-circuit between the actuators relay wiring and the positive supply or ground.
DESCRIZIONE2_3=Replace XXX ECU.
DESCRIZIONE3_1=Check wiring on Gas and Solenoid valves injectors supply.
DESCRIZIONE3_2=Check the absence of short-circuit between the actuators relay wiring and the positive supply or ground.
DESCRIZIONE3_3=Replace XXX ECU.
[P1180]
NOME=TGAS sensor
U_MIS=°C
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check TGAS sensor connector
DESCRIZIONE0_2=Check the absence of short-circuit between TGAS signal wire and negative supply
DESCRIZIONE0_3=Replace TGAS sensor
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE1_1=Check TGAS sensor connector
DESCRIZIONE1_2=Check the absence of short-circuit between TGAS signal wire and positive supply
DESCRIZIONE1_3=Check TGAS signal wire continuity from the sensor to the XXX ECU connector.
DESCRIZIONE1_4=Replace TGAS sensor
DESCRIZIONE1_5=Replace XXX ECU.
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check TGAS sensor setting
DESCRIZIONE3_2=Check the installed sensor be the suitable one.
DESCRIZIONE3_3=If you have a non-reasonable-error on engine water temperature sensor too, follow the same indications suitable for the P1115 error
DESCRIZIONE3_4=If you have an error on the sensors supply tension, follow the same indications suitable for the P1608 error.
DESCRIZIONE3_5=Replace gas temperature sensor.
DESCRIZIONE3_6=Replace XXX ECU.
[P1190]
NOME=P1 sensor
U_MIS=mbar
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check P1 sensor connector
DESCRIZIONE0_2=Check the absence of short-circuit between P1 signal wire and positive supply
DESCRIZIONE0_3=Replace P1 sensor
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE1_1=Check P1 sensor connector
DESCRIZIONE1_2=Check the absence of short-circuit between P1 signal wire and negative supply
DESCRIZIONE1_3=Check P1 signal wire continuity from the sensor to the XXX ECU connector.
DESCRIZIONE1_4=Replace P1 pressure sensor.
DESCRIZIONE1_5=Replace XXX ECU.
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check P1 sensor setting
DESCRIZIONE3_2=Check the installed sensor be the suitable one.
DESCRIZIONE3_3=If you have a non-reasonable-error on MAP pressure sensor too, follow the same indications suitable for P1105 error
DESCRIZIONE3_4=If you have an error on the TPS throttle potentiometer sensor too, follow the same indications suitable for the P1120 error
DESCRIZIONE3_5=If you have an error on the sensors supply tension too, follow the same indications suitable for the P1608 error
DESCRIZIONE3_6=Replace P1 sensor
DESCRIZIONE3_7=Replace XXX ECU.
[P1201]
NOME=1 GAS cylinder injector control
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check injectors connectors
DESCRIZIONE0_2=Check the absence of short-circuit between injectors wiring and positive supply
DESCRIZIONE0_3=Check injectors impedance (between 1 and 2 ohm).
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE0_5=Replace injectors
DESCRIZIONE1_1=Check injectors connectors
DESCRIZIONE1_2=Check the absence of short-circuit between wiring and negative supply
DESCRIZIONE1_3=Check injectors wiring continuity from the injector connector to the XXX ECU connector.
DESCRIZIONE1_4=Check injectors impedance (between 1 and 2 ohm).
DESCRIZIONE1_5=Replace XXX ECU.
DESCRIZIONE1_6=Replace injectors
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1202]
NOME=2 GAS cylinder injector control
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check injectors connectors
DESCRIZIONE0_2=Check the absence of short-circuit between injectors wiring and positive supply
DESCRIZIONE0_3=Check injectors impedance (between 1 and 2 ohm).
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE0_5=Replace injectors
DESCRIZIONE1_1=Check injectors connectors
DESCRIZIONE1_2=Check the absence of short-circuit between injectors wiring and negative supply
DESCRIZIONE1_3=Check injectors wiring continuity from the injector connector to the XXX ECU connector.
DESCRIZIONE1_4=Check injectors impedance (between 1 and 2 ohm).
DESCRIZIONE1_5=Replace XXX ECU.
DESCRIZIONE1_6=Replace injectors
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1203]
NOME=3 GAS cylinder injector control
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check injectors connectors
DESCRIZIONE0_2=Check the absence of short-circuit between injectors wiring and positive supply
DESCRIZIONE0_3=Check injectors impedance (between 1 and 2 ohm).
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE0_5=Replace injectors
DESCRIZIONE1_1=Check injectors connectors
DESCRIZIONE1_2=Check the absence of short-circuit between injectors wiring and negative supply
DESCRIZIONE1_3=Check injectors wiring continuity from the injector connector to the XXX ECU connector.
DESCRIZIONE1_4=Check injectors impedance (between 1 and 2 ohm).
DESCRIZIONE1_5=Replace XXX ECU.
DESCRIZIONE1_6=Replace injectors
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1204]
NOME=4 GAS cylinder injector control
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check injectors connectors
DESCRIZIONE0_2=Check the absence of short-circuit between injectors wiring and positive supply
DESCRIZIONE0_3=Check injectors impedance (between 1 and 2 ohm).
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE0_5=Replace injectors
DESCRIZIONE1_1=Check injectors connectors
DESCRIZIONE1_2=Check the absence of short-circuit between injectors wiring and negative supply
DESCRIZIONE1_3=Check injectors wiring continuity from the injector connector to the XXX ECU connector.
DESCRIZIONE1_4=Check injectors impedance (between 1 and 2 ohm).
DESCRIZIONE1_5=Replace XXX ECU.
DESCRIZIONE1_6=Replace injectors
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1205]
NOME=5 GAS cylinder injector control
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check injectors connectors
DESCRIZIONE0_2=Check the absence of short-circuit between injectors wiring and positive supply
DESCRIZIONE0_3=Check injectors impedance (between 1 and 2 ohm).
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE0_5=Replace injectors
DESCRIZIONE1_1=Check injectors connectors
DESCRIZIONE1_2=Check the absence of short-circuit between injectors wiring and negative supply
DESCRIZIONE1_3=Check injectors wiring continuity from the injector connector to the XXX ECU connector.
DESCRIZIONE1_4=Check injectors impedance (between 1 and 2 ohm).
DESCRIZIONE1_5=Replace XXX ECU.
DESCRIZIONE1_6=Replace injectors
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1206]
NOME=6 GAS cylinder injector control
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check injectors connectors
DESCRIZIONE0_2=Check the absence of short-circuit between injectors wiring and positive supply
DESCRIZIONE0_3=Check injectors impedance (between 1 and 2 ohm).
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE0_5=Replace injectors
DESCRIZIONE1_1=Check injectors connectors
DESCRIZIONE1_2=Check the absence of short-circuit between injectors wiring and negative supply
DESCRIZIONE1_3=Check injectors wiring continuity from the injector connector to the XXX ECU connector.
DESCRIZIONE1_4=Check injectors impedance (between 1 and 2 ohm).
DESCRIZIONE1_5=Replace XXX ECU.
DESCRIZIONE1_6=Replace injectors
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1207]
NOME=7 GAS cylinder injector control
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check injectors connectors
DESCRIZIONE0_2=Check the absence of short-circuit between injectors wiring and positive supply
DESCRIZIONE0_3=Check injectors impedance (between 1 and 2 ohm).
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE0_5=Replace injectors
DESCRIZIONE1_1=Check injectors connectors
DESCRIZIONE1_2=Check the absence of short-circuit between injectors wiring and negative supply
DESCRIZIONE1_3=Check injectors wiring continuity from the injector connector to the XXX ECU connector.
DESCRIZIONE1_4=Check injectors impedance (between 1 and 2 ohm).
DESCRIZIONE1_5=Replace XXX ECU.
DESCRIZIONE1_6=Replace injectors
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1208]
NOME=8 GAS cylinder injector control
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check injectors connectors
DESCRIZIONE0_2=Check the absence of short-circuit between injectors wiring and positive supply
DESCRIZIONE0_3=Check injectors impedance (between 1 and 2 ohm).
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE0_5=Replace injectors
DESCRIZIONE1_1=Check injectors connectors
DESCRIZIONE1_2=Check the absence of short-circuit between injectors wiring and negative supply
DESCRIZIONE1_3=Check injectors wiring continuity from the injector connector to the XXX ECU connector.
DESCRIZIONE1_4=Check injectors impedance (between 1 and 2 ohm).
DESCRIZIONE1_5=Replace XXX ECU.
DESCRIZIONE1_6=Replace injectors
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1230]
NOME=Actuators relay control
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check actuators relay wiring.
DESCRIZIONE0_2=Check the absence of short-circuit between actuators relay wiring and positive supply
DESCRIZIONE0_3=Replace actuators relay
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE1_1=Check actuators relay wiring.
DESCRIZIONE1_2=Check the absence of short-circuit between actuators relay wiring and negative supply
DESCRIZIONE1_3=Check actuators relay wiring continuity from its connector to the XXX ECU one.
DESCRIZIONE1_4=Replace actuators relay
DESCRIZIONE1_5=Replace XXX ECU.
DESCRIZIONE2_1=Check actuators relay wiring.
DESCRIZIONE3_1=Check actuators relay wiring.
DESCRIZIONE3_2=Check absence of short-circuit between actuators relay wiring and positive supply or GND (ground)
DESCRIZIONE3_3=Check injectors and solenoid valves connectors
DESCRIZIONE3_4=Replace actuators relay
DESCRIZIONE3_5=Replace XXX ECU.
[P1231]
NOME=GAS 1 solenoid valves control
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check GAS solenoid valves wiring
DESCRIZIONE0_2=Check the absence of short-circuit between GAS solenoid valve wiring and positive supply
DESCRIZIONE0_3=Check GAS solenoid valve wiring continuity from its connector to the XXX ECU one.
DESCRIZIONE0_4=Replace GAS solenoid valve wiring
DESCRIZIONE0_5=Replace GAS solenoid valve
DESCRIZIONE0_6=Replace XXX ECU.
DESCRIZIONE1_1=Check GAS solenoid valve wiring
DESCRIZIONE1_2=Check the absence of short-circuit between GAS solenoid valve wiring and negative supply.
DESCRIZIONE1_3=Check the Gas solenoid valve wiring continuity from its connector to the XXX ECU one.
DESCRIZIONE1_4=Replace Gas solenoid valve
DESCRIZIONE1_5=Replace XXX ECU.
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1232]
NOME=GAS 2 solenoid valves control
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check GAS solenoid valves wiring
DESCRIZIONE0_2=Check the absence of short-circuit between GAS solenoid valve wiring and positive supply
DESCRIZIONE0_3=Check GAS solenoid valve wiring continuity from its connector to the XXX ECU one.
DESCRIZIONE0_4=Replace GAS solenoid valve wiring
DESCRIZIONE0_5=Replace GAS solenoid valve
DESCRIZIONE0_6=Replace XXX ECU.
DESCRIZIONE1_1=Check GAS solenoid valve wiring
DESCRIZIONE1_2=Check the absence of short-circuit between GAS solenoid valve wiring and negative supply.
DESCRIZIONE1_3=Check GAS solenoid valve wireing continuity from its connector to the XXX ECU one.
DESCRIZIONE1_4=Replace GAS solenoid valve
DESCRIZIONE1_5=Replace XXX ECU.
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1233]
NOME=GAS 3 solenoid valves control
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check GAS solenoid valve wiring
DESCRIZIONE0_2=Check the absence of short-circuit between GAS solenoid valve wiring and positive supply
DESCRIZIONE0_3=Check GAS solenoid valve wiring continuity from its connector to the XXX ECU one.
DESCRIZIONE0_4=Replace GAS solenoid valve wiring
DESCRIZIONE0_5=Replace GAS solenoid valve
DESCRIZIONE0_6=Replace XXX ECU.
DESCRIZIONE1_1=Check GAS solenoid valve wiring
DESCRIZIONE1_2=Check the absence of short-circuit between GAS solenoid valve wiring and negative supply.
DESCRIZIONE1_3=Check GAS solenoid valve wiring continuity from its connector to the XXX ECU one.
DESCRIZIONE1_4=Replace GAS solenoid valve
DESCRIZIONE1_5=Replace XXX ECU.
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1234]
NOME=GAS 4 solenoid valves control
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check GAS solenoid valve wiring
DESCRIZIONE0_2=Check the absence of short-circuit between GAS solenoid valve wiring and positive supply
DESCRIZIONE0_3=Check GAS solenoid valve wiring continuity from its connector to the XXX ECU one.
DESCRIZIONE0_4=Replace GAS solenoid valves wiring
DESCRIZIONE0_5=Replace GAS solenoid valve
DESCRIZIONE0_6=Replace XXX ECU.
DESCRIZIONE1_1=Check GAS solenoid valve wiring
DESCRIZIONE1_2=Check the absence of short-circuit between GAS solenoid valve wiring and negative supply.
DESCRIZIONE1_3=Check GAS solenoid valve wiring continuity from its connector to the XXX ECU one.
DESCRIZIONE1_4=Replace GAS solenoid valve
DESCRIZIONE1_5=Replace XXX ECU.
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1248]
NOME=Inertial switch inlet
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check inertial switch wiring
DESCRIZIONE0_2=Check the absence of short-circuit between inertial switch wiring and positive supply
DESCRIZIONE0_3=Replace XXX ECU.
DESCRIZIONE1_1=Check inertial switch wiring
DESCRIZIONE1_2=Check the absence of short-circuit between inertial switch wiring and the negative supply
DESCRIZIONE1_3=Check inertial switch wiring continuity from its connector (or taking point) to the XXX ECU one.
DESCRIZIONE1_4=Replace XXX ECU.
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1263]
NOME=Petrol cylinder 1 injector
U_MIS=
U_MISC=mV
U_MIT=s
AGGIUNTIVINOME.0=TPS 100% Threshold
AGGIUNTIVIU_MIS.0=%
AGGIUNTIVINOME.1=RPM 100%Threshold
AGGIUNTIVIU_MIS.1=RPM
AGGIUNTIVINOME.2=TPS cut-off Threshold
AGGIUNTIVIU_MIS.2=%
AGGIUNTIVINOME.3=RPM cut-off Threshold
AGGIUNTIVIU_MIS.3=RPM
DESCRIZIONE0_1=Check injectors connectors
DESCRIZIONE0_2=Check the absence of short-circuit between injectors wiring and GND
DESCRIZIONE0_3=Check injector wiring continuity from the injector connector (or taking point) to the XXX ECU connector.
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check injectors connectors
DESCRIZIONE3_2=Check the absence of short-circuit between injectors wiring and the supplies.
DESCRIZIONE3_3=Check injectors wiring continuity from the injector connector (or taking point) to the XXX ECU one
DESCRIZIONE3_4=Replace XXX ECU.
[P1266]
NOME=Petrol cylinder 2 injector
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check injectors connectors
DESCRIZIONE0_2=Check the absence of short-circuit between injectors wiring and GND
DESCRIZIONE0_3=Check injector wiring continuity from the injector connector (or taking point) to the XXX ECU connector.
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check injectors connectors
DESCRIZIONE3_2=Check the absence of short-circuit between injectors wiring and the supplies.
DESCRIZIONE3_3=Check injectors wiring continuity from the injector connector (or taking point) to the XXX ECU connector.
DESCRIZIONE3_4=Replace XXX ECU.
[P1269]
NOME=Petrol cylinder 3 injector
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check injectors connectors
DESCRIZIONE0_2=Check the absence of short-circuit between injectors wiring and GND
DESCRIZIONE0_3=Check injector wiring continuity from the injector connector (or taking point) to the XXX ECU connector.
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check injectors connectors
DESCRIZIONE3_2=Check the absence of short-circuit between injectors wiring and the supplies.
DESCRIZIONE3_3=Check injectors wiring continuity from the injector connector (or taking point) to the XXX ECU collector.
DESCRIZIONE3_4=Replace XXX ECU.
[P1272]
NOME=Petrol cylinder 4 injector
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check injectors connectors
DESCRIZIONE0_2=Check the absence of short-circuit between injectors wiring and GND.
DESCRIZIONE0_3=Check injector wiring continuity from the injector connector (or taking point) to the XXX ECU connector.
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check injectors connectors
DESCRIZIONE3_2=Check the absence of short-circuit between injectors wiring and the supplies.
DESCRIZIONE3_3=Check injectors wiring continuity from the injector connector (or taking point) to the XXX ECU collector.
DESCRIZIONE3_4=Replace XXX ECU.
[P1275]
NOME=Petrol cylinder 5 injector
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check injectors connectors
DESCRIZIONE0_2=Check the absence of short-circuit between injectors wiring and GND.
DESCRIZIONE0_3=Check injector wiring continuity from the injector connector (or taking point) to the XXX ECU connector.
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check injectors connectors
DESCRIZIONE3_2=Check the absence of short-circuit between injectors wiring and the supplies.
DESCRIZIONE3_3=Check injectors wiring continuity from the injector connector (or taking point) to the XXX ECU collector.
DESCRIZIONE3_4=Replace XXX ECU.
[P1278]
NOME=Petrol cylinder 6 injector
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check injectors connectors
DESCRIZIONE0_2=Check the absence of short-circuit between injectors wiring and GND.
DESCRIZIONE0_3=Check continuity of injector wire from its connector (or connection point) to the XXX ECU connector.
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check injectors connectors
DESCRIZIONE3_2=Check the absence of short-circuit between injectors wiring and the supplies.
DESCRIZIONE3_3=Check injectors wiring continuity from the injector connector (or taking point) to the XXX ECU collector.
DESCRIZIONE3_4=Replace XXX ECU.
[P1281]
NOME=Petrol cylinder 7 injector
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check injectors connectors
DESCRIZIONE0_2=Check the absence of short-circuit between injectors wiring and GND.
DESCRIZIONE0_3=Check injector wiring continuity from the injector connector (or taking point) to the XXX ECU connector.
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check injectors connectors
DESCRIZIONE3_2=Check the absence of short-circuit between injectors wiring and the supplies.
DESCRIZIONE3_3=Check injectors wiring continuity from the injector connector (or taking point) to the XXX ECU collector.
DESCRIZIONE3_4=Replace XXX ECU.
[P1284]
NOME=Petrol cylinder 8 injector
U_MIS=
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check injectors connectors
DESCRIZIONE0_2=Check the absence of short-circuit between injectors wiring and GND.
DESCRIZIONE0_3=Check injector wiring continuity from the injector connector (or taking point) to the XXX ECU connector.
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check injectors connectors
DESCRIZIONE3_2=Check the absence of short-circuit between injectors wiring and the supplies.
DESCRIZIONE3_3=Check injectors wiring continuity from the injector connector (or taking point) to the XXX ECU collector.
DESCRIZIONE3_4=Replace XXX ECU.
[P1335]
NOME=rpm or cranck shaft signal
U_MIS=rpm
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check setting parameters and correct connection for the RPM signal.
DESCRIZIONE0_2=Check RPM wire/wires continuity from the signal taking point to the XXX ECU connector.
DESCRIZIONE0_3=Replace XXX ECU.
DESCRIZIONE1_1=Check setting parameters and correct connection for the RPM signal.
DESCRIZIONE1_2=Check RPM wire/wires continuity from the signal taking point to the XXX ECU connector.
DESCRIZIONE1_3=Replace XXX ECU.
DESCRIZIONE2_1=Check signal taking point is correct.
DESCRIZIONE2_2=Check rpm or cranck shaft signal wiring from the taking point to the XXX ECU connector.
DESCRIZIONE2_3=Replace XXX ECU.
DESCRIZIONE3_1=Check signal taking point is correct.
DESCRIZIONE3_2=Check rpm or cranck shaft signal setting
DESCRIZIONE3_3=Check the absence of short-circuit between rpm or cranck shaft signal wiring and the supplies.
DESCRIZIONE3_4=Replace XXX ECU.
[P1420]
NOME=POSTCAT signal
U_MIS=mV
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check lambda oxygen sensor signal has been correctly taken.
DESCRIZIONE0_2=Check the absence of short-circuit between POSTCAT lambda oxygen sensor signal wire and the supplies.
DESCRIZIONE0_3=Replace XXX ECU.
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check lambda oxygen sensor signal has been correctly taken.
DESCRIZIONE3_2=Check POSTCAT lambda oxygen sensor signal wire continuity from its connector (or signal taking point) to XXX ECU collector..
DESCRIZIONE3_3=Check sensor setting
DESCRIZIONE3_4=Replace XXX ECU.
[P1421]
NOME=POSTCAT ground
U_MIS=mV
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=NOT SUPPORTED
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check POSTCAT lambda oxygen sensor ground taking point is correct.
DESCRIZIONE3_2=Check the absence of short-circuit between POSTCAT lambda oxygen sensor ground wire and the positive supply.
DESCRIZIONE3_3=Check sensor setting
DESCRIZIONE3_4=Replace XXX ECU.
[P1460]
NOME=Gas level signal
U_MIS=1/1000
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check level sensor connector.
DESCRIZIONE0_2=Check the absence of short-circuit between level sensor wiring and positive supply.
DESCRIZIONE0_3=Check level sensor wiring continuity up to the XXX ECU connector.
DESCRIZIONE0_4=Check level sensor setting
DESCRIZIONE0_5=Check BRC sensor installed be the suitable one.
DESCRIZIONE0_6=If you have an error on the sensor supply tension, follow the same indications suitable for error P1608.
DESCRIZIONE0_7=Replace level sensor.
DESCRIZIONE0_8=Replace XXX ECU.
DESCRIZIONE1_1=Check level sensor connector
DESCRIZIONE1_2=Check the absence of short-circuit between level sensor wiring and negative supply.
DESCRIZIONE1_3=Check level sensor wiring continuity up to the XXX ECU connector.
DESCRIZIONE1_4=Check level sensor setting
DESCRIZIONE1_5=Check BRC sensor installed be the suitable one.
DESCRIZIONE1_6=If you have an error on the sensor supply tension, follow the same indications suitable for error P1608.
DESCRIZIONE1_7=Replace level sensor.
DESCRIZIONE1_8=Replace XXX ECU.
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1560]
NOME=Battery voltage
U_MIS=mV
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check battery supply wiring.
DESCRIZIONE0_2=Check supply wiring continuity (positive battery and ground) from the taking point to the XXX ECU connector.
DESCRIZIONE0_3=Check battery voltage with a voltmeter
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE1_1=Check battery supply wiring.
DESCRIZIONE1_2=Check supply wiring continuity (positive battery and ground) from the taking point to the XXX ECU connector.
DESCRIZIONE1_3=Check battery voltage with a voltmeter
DESCRIZIONE1_4=Replace XXX ECU.
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1608]
NOME=Sensors supply tension
U_MIS=mV
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check sensors supply tension wiring.
DESCRIZIONE0_2=Check sensors supply tension wiring from XXX ECU to the different sensors connectors.
DESCRIZIONE0_3=Check XXX ECU fuses continuity.
DESCRIZIONE0_4=Check sensors supply tension coming out from the XXX ECU with a voltmeter.
DESCRIZIONE0_5=Replace XXX ECU.
DESCRIZIONE1_1=Check sensors supply tension wiring.
DESCRIZIONE1_2=Check sensors supply tension wiring from XXX ECU to the different sensors connectors.
DESCRIZIONE1_3=Check XXX ECU fuses continuity.
DESCRIZIONE1_4=Check sensors supply tension coming out from the XXX ECU with a voltmeter.
DESCRIZIONE1_5=Replace XXX ECU.
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1600]
NOME=K line
U_MIS=
U_MISC=
U_MIT=s
DESCRIZIONE0_1=NOT SUPPORTED
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1601]
NOME=EEPROM diagnosis
U_MIS=
U_MISC=
U_MIT=s
DESCRIZIONE0_1=NOT SUPPORTED
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1604]
NOME=RAM diagnosis
U_MIS=
U_MISC=
U_MIT=s
DESCRIZIONE0_1=NOT SUPPORTED
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1605]
NOME=FLASH diagnosis
U_MIS=
U_MISC=
U_MIT=s
DESCRIZIONE0_1=NOT SUPPORTED
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1606]
NOME=Microprocessor Diagnosis
U_MIS=
U_MISC=
U_MIT=s
DESCRIZIONE0_1=NOT SUPPORTED
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=NOT SUPPORTED
[P1649]
NOME=CAN Line
U_MIS=
U_MISC=
U_MIT=s
DESCRIZIONE0_1=NOT SUPPORTED
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=Check signal taking point is correct.
DESCRIZIONE2_2=Check CAN-BUS signal wiring from the taking point to the XXX ECU connector.
DESCRIZIONE2_3=Replace XXX ECU.
DESCRIZIONE3_1=Check signal taking point is correct.
DESCRIZIONE3_2=Check the absence of short-circuit between CAN-BUS signal wiring and the supplies.
DESCRIZIONE3_3=Replace XXX ECU.
[P1191]
NOME=P1 bis sensor
U_MIS=mbar
U_MISC=mV
U_MIT=s
DESCRIZIONE0_1=Check P1bis sensor connector
DESCRIZIONE0_2=Check the absence of short-circuit between P1bis signal wire and positive supply
DESCRIZIONE0_3=Replace P1bis sensor
DESCRIZIONE0_4=Replace XXX ECU.
DESCRIZIONE1_1=Check P1bis sensor connector
DESCRIZIONE1_2=Check the absence of short-circuits between the P1bis signal wire and negative supply.
DESCRIZIONE1_3=Check P1bis signal wiring continuity from the sensor to the XXX ECU connector.
DESCRIZIONE1_4=Replace P1bis pressure sensor.
DESCRIZIONE1_5=Replace XXX ECU.
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Chech P1bis sensor setting
DESCRIZIONE3_2=Check the correct sensor be installed.
DESCRIZIONE3_3=If you have a non-plausibile-error on the MAP pressure sensor too, follow the same indications suitable for error P1105
DESCRIZIONE3_4=If you have an error on the TPS throttle potentiometer sensor too, follow the same indications suitable for error P1120
DESCRIZIONE3_5=If you have an error on the sensor supply tension too, follow the same indications suitable for error P1608
DESCRIZIONE3_6=Replace P1bis sensor.
DESCRIZIONE3_7=Replace XXX ECU.
[P1650]
NOME=petrol-gas change-over switch
U_MIS=
U_MISC=
U_MIT=s
DESCRIZIONE0_1=check gas/petrol change-over switch connector.
DESCRIZIONE0_2=check the absence of short-circuits between the change-over switch wire and the supply.
DESCRIZIONE0_3=Check change-over switch wire continuity from its connector up to the XXX ECU connector.
DESCRIZIONE0_4=If you have an error on the sensor supply tension, follow the same indications suitable for error P1608
DESCRIZIONE0_5=Replace gas/petrol change-over switch.
DESCRIZIONE0_6=Replace XXX ECU.
DESCRIZIONE1_1=NOT SUPPORTED
DESCRIZIONE2_1=NOT SUPPORTED
DESCRIZIONE3_1=Check the absence of short-circuit between change-over switch wiring and the supply.
DESCRIZIONE3_2=Check change-over switch wiring continuity.
DESCRIZIONE3_3=Check change-over switch wiring connector.
DESCRIZIONE3_4=Replace change-over switch.
[AGGIUNTIVI_1]
NOME=MAP max for engine off
U_MIS=mbar
[AGGIUNTIVI_2]
NOME=Not used
U_MIS=
[AGGIUNTIVI_3]
NOME=Not used
U_MIS=
[AGGIUNTIVI_4]
NOME=Time since Gas changeover
U_MIS=ms
[AGGIUNTIVI_5]
NOME=Max difference between TGAS and TH2O
U_MIS=°C
[AGGIUNTIVI_6]
NOME=Not used
U_MIS=
[AGGIUNTIVI_7]
NOME=Not used
U_MIS=
[AGGIUNTIVI_8]
NOME=Not used
U_MIS=
[AGGIUNTIVI_9]
NOME=Not used
U_MIS=
[AGGIUNTIVI_10]
NOME=Not used
U_MIS=
[AGGIUNTIVI_11]
NOME=Not used
U_MIS=
[AGGIUNTIVI_12]
NOME=Not used
U_MIS=
[AGGIUNTIVI_13]
NOME=OxyVoltCutOff
U_MIS=mV
[AGGIUNTIVI_14]
NOME=Min RPM reasonable
U_MIS=rpm
[AGGIUNTIVI_15]
NOME=Max RPM reasonable
U_MIS=rpm
[AGGIUNTIVI_16]
NOME=Not used
U_MIS=
[AGGIUNTIVI_17]
NOME=Not used
U_MIS=
[AGGIUNTIVI_18]
NOME=Not used
U_MIS=
[AGGIUNTIVI_19]
NOME=P1-MAP min
U_MIS=mbar
[AGGIUNTIVI_20]
NOME=P1-MAP max
U_MIS=mbar
[AGGIUNTIVI_21]
NOME=Delay since key contact
U_MIS=ms
[AGGIUNTIVI_22]
NOME=Window for petrol injectors check
U_MIS=n[rpm]
[AGGIUNTIVI_23]
NOME=Difference nr. of injections
U_MIS=
[AGGIUNTIVI_24]
NOME=Difference VKEY - VACT
U_MIS=mV
[AGGIUNTIVI_25]
NOME=Time between two beeps in petrol mode
U_MIS=s
[AGGIUNTIVI_26]
NOME=Number of Beeps in petrol mode
U_MIS=
[AGGIUNTIVI_27]
NOME=Blinking led for diagnostic in petrol mode
U_MIS=
[AGGIUNTIVI_28]
NOME=Time between two beeps in gas mode
U_MIS=s
[AGGIUNTIVI_29]
NOME=Number of Beeps in gas mode
U_MIS=
[AGGIUNTIVI_30]
NOME=Blinking led for diagnostic in gas mode
U_MIS=
[AGGIUNTIVI_31]
NOME=Ton petrol min
U_MIS=ms
[AGGIUNTIVI_32]
NOME=Ton petrol max
U_MIS=ms
[AGGIUNTIVI_33]
NOME=Window for VCH signal stability check
U_MIS=ms
[AGGIUNTIVI_34]
NOME=Time since vehicle stall
U_MIS=ms
